{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":104,"n_cols":3,"rows_kept":104,"cut":false,"hidden":false,"merged":[]}
[]
[null,"845C","865C"]
["ENGINE"]
["Make / Model  ","FPT / F4HE613B*W002","FPT / F4HE613B*W002"]
["Type ","Electronic common rail fuel system, Water cooled,4 Cycle, Direct injection, Open combustion chamber, Turbocharged, Charge air cooled. Tier IV","Electronic common rail fuel system, Water cooled,4 Cycle, Direct injection, Open combustion chamber, Turbocharged, Charge air cooled. Tier IV"]
["Cylinders ",6,6]
["Bore/Stroke ","104 mm X 132 mm (4.09 in x 5.17 in)","104 mm X 132 mm (4.09 in x 5.17 in)"]
["Displacement ","6.7 L (409 Cubic Inch)","6.7 L (409 Cubic Inch)"]
["Horsepower at 2200 rpm Gross (SAE J1995 Gross) - Low Curve ","112 kW/ 150 hp","144 kW/ 193 hp"]
["Horsepower at 2200 rpm Gross (SAE J1995 Gross) - High Curve ","129 kW/ 173 hp","164 kW/ 220 hp"]
["Horsepower at 2200 rpm Gross (SAE J1995 Gross) - Mid Curve ","-","153 kW/ 205 hp"]
["Horsepower at 2200 rpm Net (SAE J1349) - Low Curve ","104 kW/ 140 hp","133 kW/ 178 hp"]
["Horsepower at 2200 rpm Net (SAE J1349) - Mid Curve ","-","142 kW/ 190 hp"]
["Horsepower at 2200 rpm Net (SAE J1349) - High Curve ","119 kW/ 160 hp","153 kW/ 205 hp"]
["maximum torque at 1500 rpm gross (sae j1995 gross) - Low Curve ","659 Nm (486 ft.lb)","830 Nm (612 ft.lb)"]
["Maximum torque at 1500 rpm Gross (SAE J1995 Gross) - Mid Curve ","-","880 Nm (649 ft.lb)"]
["Maximum torque at 1500 rpm Gross (SAE J1995 Gross) - High Curve ","758 Nm (560 ft.lb)","930 Nm (686 ft.lb)"]
["Maximum torque at 1500 rpm Net (SAE J1349) - Low Curve ","591 Nm (436 ft.lb)","743 Nm (548 ft.lb)"]
["Maximum torque at 1500 rpm Net (SAE J1349) - High Curve ","678 Nm (500 ft.lb)","832 Nm (615 ft.lb)"]
["POWERTRAIN"]
["Rear axle - Vertical ground clearance ","380 mm (14.9\")","380 mm (14.9\")"]
["Rear axle - Differential ","Limited Slip","Limited Slip"]
["Rear axle - Brakes ","Disc, bathed in Oil","Disc, bathed in Oil"]
["Rear axle - Number of disks per brake ",5,5]
["Tandem - Type ","Welded Plate","Welded Plate"]
["Tandem - Oscillation ","20 Deg in each direction","20 Deg in each direction"]
["Tandem - Command chain pitch ","50.8 mm pitch (2.00\"), press fit connecting link","50.8 mm pitch (2.00\"), press fit connecting link"]
["Tandem - Thickness of the internal and external side wall ","/","19 mm"]
["Front axle - Type ","CNH LA","CNH LA"]
["Front axle - Oscillation ","15 deg each way","15 deg each way"]
["Front axle - Wheel lean ","20°","20°"]
["Front axle - Ground clearance ","580 mm","580 mm"]
["SYSTEM"]
["Type ","Piston pump, variable displacement. Pressure and flow compensated, Load sensing","Piston pump, variable displacement. Pressure and flow compensated, Load sensing"]
["Hydraulic pump ","Rexroth","Rexroth"]
["Rated flow ","186 LPM (49 GPM) @ 2200 RPM","186 LPM (49 GPM) @ 2200 RPM"]
["Control valve ","HUSCO, LOAD SENSING 9 SECTION","HUSCO, LOAD SENSING 9 SECTION"]
["ELECTRICAL SYSTEM"]
["Power  ","24V","24V"]
["Alternator  ","BOSCH - 120A","BOSCH - 120A"]
["Batteries  ","2x100 Ah – low maintenance","2x100 Ah – low maintenance"]
["BLADE/MOLDBOARD"]
["Type ","Standard/Optional","Standard/Optional"]
["Form ","Involute curve","Involute curve"]
["Width ","3962 mm - standard, 3658 mm/ 4267 mm - optional","standard 3962 mm / optional 3658-4267 mm"]
["Height of dozer blade (curved profile) ","953 mm (37.5\")","622 mm"]
["Thickness ","22 mm (0.875\")","22 mm (875\")"]
["Cutting edge ","2 interchangeable","2 interchangeable"]
["Blade pitch positions - Normal pitch  ","47°","47°"]
["Maximum pitch ","87°","87°"]
["Blade side shift - Right ","1105 mm (43.5\")","1257 mm (49.5\")"]
["Blade side shift - Left ","1105 mm (43.5\")","1105 mm (43.5\")"]
["Maximum bank-cutting angle (left and right) ","  90°","90°"]
["Ground penetration (max.)  ","711.2 mm (28\")","711.2 mm (28\")"]
["Lift above ground (max.)  ","444.5 mm (17.5\")","444.5 mm (17.5\")"]
["Blade side shift and pitch  ","Hydraulic type","Hydraulic type"]
["STEERING"]
["Type ","Hydrostatic power steering","Hydrostatic power steering"]
["Steering wheel turns (lock to lock)  ","4.5 turns (fast), 3.2 turns (slow)","4.5 turns (fast), 3.2 turns (slow)"]
["Pump capacity  ","41.8 LPM (11.1GPM) @ 2200 engine RPM","41.8 LPM (11.1GPM) @ 2200 engine RPM"]
["Pressure ","175 bar (2530 PSI) Integral with priority valve","175 bar (2530 PSI) Integral with priority valve"]
["Cylinders ",2,2]
["ARTICULATION"]
["Type ","Hydraulic actuated (with lock valve)","Hydraulic actuated (with lock valve)"]
["Angle ","25° left/right","25° left/right"]
["Controls ","Hydraulic","Hydraulic"]
["CAPACITIES (REFILL)"]
["Engine with and w/o filter ","16/15 L","16/15 L"]
["Fuel tank ","380 L","380 L"]
["DEF tank ","60 L","60 L"]
["Transmission with and w/o filter ","31/30 L","31/30 L"]
["Engine water cooling system ","16 L","16 L"]
["Hydraulic oil tank ","90 L","90 L"]
["Total hydraulic system ","158 L","158 L"]
["Rear axle center ","44 L","44 L"]
["Tandem case (each) ","69 L","69 L"]
["SADDLE"]
["Locking system ","5 Positions, Two cylinders actuated by an electric","5 Positions, Two cylinders actuated by an electric"]
["FRAME"]
["Type ","Box section","Box section"]
["Size - Rear sectionn ","254x298 mm","327 X 220.5 mm"]
["Size - Front section ","190x327 mm","298 X 258 mm"]
["DRAWBAR"]
["Type ","“A” frame welded construction with center mounted circle turn motor. Shim adjustable at ball and circle","“A” frame welded construction with center mounted circle turn motor. Shim adjustable at ball and circle"]
["CIRCLE"]
["Type ","Welded construction","Welded construction"]
["Maximum ouside diameter ","1752.6 mm (69\")","1752.6 mm (69\")"]
["Rotation / Speed ","360°/ 1.2 RPM (7.2 degrees per second)","360°/ 1.2 RPM (7.2 degrees per second)"]
["Nº of supports in phenolic resin ",4,4]
["REAR RIPPER"]
["Type ","Parallelogram","Parallelogram"]
["Cutting width ","2156 mm (85.3\")","2195 mm (86.4\")"]
["Ripper teeth ",5,"3 STD / 5 OPT"]
["Lift above ground - Ripper teeth ","703 mm (27.67\")","518 mm (20.38\")"]
["Maximum penetration - Ripper teeth ","306 mm (12.1\")","437 mm (17.22\")"]
["Weight  ","640 kg (1410 lb)","795 kg"]
["FRONT SCARIFIER"]
["Cutting width ","1168 mm","1168 mm"]
["Teeth ","5 (opt, 11)","5 STD / 11 OPT"]
["Spacing between teeth ","229 mm (opt, 114.5 mm)","229 mm (opt, 114.5 mm)"]
["Lift above ground ","527 mm","527 mm"]
["Maximum penetration  ","318 mm","318 mm"]
["Weight  ","570 kg","570 kg"]
["Scarifier teeth  ","5 STD / 9 OPT","-"]