{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":61,"n_cols":19,"rows_kept":61,"cut":false,"hidden":false,"merged":[[60,0,60,20]]}
[]
[null,"CX19D","CX12D","CX14D","CX15EV","CX17D","CX18D","CX20D","CX22D","CX25EV","CX25D","CX35D","CX42D","CX45D","CX50D","CX55D","CX58D","CX60D","CX65D"]
["ENGINE"]
["Type ","YANMAR 3TNV76 - STAGE V","KUBOTA D722 - STAGE V","KUBOTA D722 - STAGE V","Internal Permanent Magnets (IPM)","YANMAR 3TNV70 - STAGE V","YANMAR 3TNV70 - STAGE V","YANMAR 3TNV76 - STAGE V","KUBOTA D1105 - STAGE V","Internal Permanent Magnets (IPM)","YANMAR 3TNV76 - STAGE V","KUBOTA D1703-M - STAGE V","KUBOTA D1803-CR-T - STAGE V","KUBOTA D1803-CR-T - STAGE V","KUBOTA V2403-CR-T - STAGE V","KUBOTA V2403-CR-T - STAGE V","KUBOTA V2607-CR-T - STAGE V","KUBOTA V2607-CR-T - STAGE V","KUBOTA V2607-CR-T - STAGE V"]
["Max. Power (kW / hp) ","(2200 rpm) 13.7 - 18.4","(2200 rpm) 8.8 - 11.8","(2200 rpm) 8.8 - 11.8","11.0 / 14.7","(2200 rpm) 12 - 16.1","(2200 rpm) 12 - 16.1","(2200 rpm) 13.7 - 18.4","(2400 rpm) 15.4 - 20.7","25.0 / 33.5","(2200 rpm) 13.7 - 18.4","(2200 rpm) 18.2 - 24.4","(2300 rpm) 32.3 - 43.3","(2300 rpm) 32.3 - 43.3","(2300 rpm) 42.6 - 57.1","(2300 rpm) 42.6 - 57.1","(2300 rpm) 44.3 - 59.4","(2300 rpm) 44.3 - 59.4","(2200 rpm) 44.3 - 59.4"]
["Displacement (cm³) ",1116,719,719,"-",854,854,1116,1105,"-",1116,1647,1826,1826,2434,2434,2615,2615,2615]
["Supply ","-","-","-","three-phase alternating current","-","-","-","-","three-phase alternating current","-","-","-","-","-","-","-","-","-"]
["Number of cylinders (n°) ",3,3,3,"-",3,3,3,3,"-",3,3,3,3,4,4,4,4,4]
["Cooling ","Liquid","Liquid","Liquid","-","Liquid","Liquid","Liquid","Liquid","-","Liquid","Liquid","Liquid","Liquid","Liquid","Liquid","Liquid","Liquid","Liquid"]
["Consumption (l/h) ",3.1,1.8,1.8,"-",2.4,2.4,3.1,3,"-",3,3.5,5.4,5.4,6.9,6.9,7.6,7.6,7.6]
["Alternator V (Ah) ","12 (40)","12 (40)","12 (40)","-","12 (40)","12 (40)","12 (40)","12 (40)","-","12 (40)","12 (40)","12 (70)","12 (70)","12 (70)","12 (70)","12 (60)","12 (60)","12 (60)"]
["Battery V (Ah) ","12 (65)","12 (45)","12 (45)","-","12 (65)","12 (65)","12 (65)","12 (62)","-","12 (65)","12 (80)","12 (74)","12 (74)","12 (100)","12 (100)","12 (95)","12 (95)","12 (95)"]
["HYDRAULIC SYSTEM"]
["Control valve ","-","-","-","Load Sensing Flow Sharing","-","-","-","-","Load Sensing Flow Sharing","-","-","-","-","-","-","-","-","-"]
["Hydraulic system capacity (l) ","-","-","-",15,"-","-","-","-",28,"-","-","-","-","-","-","-","-","-"]
["Circuit Type ","-","-","-","-","-","-","-","Load Sensing closed center system with “Flow Sharing” control valve","-","Load Sensing centre closed\nwith Flow Sharing distributor","Load Sensing closed center system with “Flow Sharing” control valve","Load Sensing closed center system with “Flow Sharing” control valve","Load Sensing closed center system with “Flow Sharing” control valve","Load Sensing closed center system with “Flow Sharing” control valve","Load Sensing\nclosed center system with\n“Flow Sharing” control valve","Load Sensing\nclosed center system with\n“Flow Sharing” control valve","Load Sensing closed center\nsystem with “Flow Sharing”\ncontrol valve","Load Sensing closed center system with “Flow Sharing” control valve"]
["Pump type ","variable flow","n°2 gear pumps","variable flow","1 Low Noise Helical Gear Pump","variable flow","variable flow","variable flow","1 LS variable pump + 1 gear pump","1 LS Variable pump","1 Load Sensing pump with\nvariable displacement","1 LS variable pump","1 LS hydraulic variable pump with electronic control + 1 gear pump","1 LS hydraulic variable pump with electronic control + 1 gear pump","LS hydraulic variable pump with electronic control + 1 gear pump","LS hydraulic variable pump\nwith electronic control\n+ 1 gear pump","LS hydraulic variable\npump with electronic\ncontrol + 1 gear pump","1 LS hydraulic variable pump\nwith electronic control\n+ 1 gear pump","1 LS hydraulic variable pump with electronic control + 1 gear pump"]
["Pump displacement (cm³) ","9 + 9 + 6.6","5.6 + 5.6","6.0 + 6.0",10.1,"8 + 8 + 6.6","8 + 8 + 6.6","9 + 9 + 6.6","25 + 5",18,25,48,"53.7 + 11.2","53.7 + 11.2","65 + 14.5","65 + 14.5","65 + 14.5","71 + 14","71 + 14"]
["Pump capacity (l/min) ","18 + 18 + 13.1","12 + 12","13 + 13","-","16 + 16 + 13.1","16 + 16 + 13.1","18 + 18 + 13.1","48 + 9.5","-",50,101,"107 + 22.3","107 + 22.3","129 + 28.8","129 + 28.8","129 + 28.8","141 + 27.8","141 + 27.8"]
["Pump flow rate (l/min) ","-","-","-",26,"-","-","-","-",46,"-","-","-","-","-","-","-","-","-"]
["Max. circuit calibration pressure (bar) ",240,170,190,180,220,220,240,240,210,250,260,280,280,280,280,280,280,280]
["Auxiliary system (max pressure) - AUX 1 single or double effect (l/min) ","31.1 - 205 bar","26 - 165 bar","28 - 200 bar","28 - 180 bar","29.1 - 205 bar","29.1 - 205 bar","31.1 - 205 bar","50 - 200 bar*","40 - 210 bar","50 - 200 / 250 bar","40 (50 Max) 200 left /\n250 right bar","50 (70 Max) - 200 left /\n280 right bar","50 (70 Max) - 200 left /\n280 right bar","60 (70 Max) - 200 left /\n280 right bar","60 (70 Max) - 200 left /\n280 right bar","70 (80 Max) - 200 left /\n280 right bar","85 - 200 bar","85 - 200 bar"]
["Auxiliary system (max pressure) - AUX 2 double effect (optional) (l/min) ","13.1 - 205 bar","12 - 165 bar","13 - 165 bar","10/7 - 180 bar","13.1 - 205 bar","13.1 - 205 bar","13.1 - 205 bar","13/8 - 220 bar","13/9 - 210 bar","12 /8 - 250 bar","32/20 - 190 (250 Max) bar","double effect - optional\n60/43 - 280 bar","60/43 - 280 bar","60/43 - 280 bar","60/43 - 280 bar","45/39 - 280 bar","65/90 - 280 bar","65/90 - 280 bar"]
["Auxiliary system (max pressure) - AUX 3 double effect (optional) (l/min) ","18 - 240 bar","-","-","-","16 - 220 bar","16 - 220 bar","18 - 240 bar","50 - 220 bar","28/24 - 210 bar","29 / 22 - 250 bar","32/20 - 190 (250 Max) bar","double effect - optional\n40/32- 280 bar","40/32 - 280 bar","40/32 - 280 bar","40/32 - 280 bar","78/58 - 280 bar","45 - 280 bar","45 - 280 bar"]
["SLEWING & TRAVEL SPEED"]
["Travelling speed (AUTO TWO SPEED) (km/h) ","1st : 0 ÷ 2.3 / 2nd : 0 ÷ 4.4","1st : 0 ÷ 1.8 / 2nd : 0 ÷ 3.8","1st : 0 ÷ 1.8 / 2nd : 0 ÷ 3.8","1st : 0 ÷ 1.8 / 2nd : 0 ÷ 3.8","1st : 0 ÷ 2.2 / 2nd : 0 ÷ 4.1","1st : 0 ÷ 2.2 / 2nd : 0 ÷ 4.1","1st : 0 ÷ 2.3 / 2nd : 0 ÷ 4.4","1st : 0 ÷ 2.6 / 2nd : 0 ÷ 4.0","1st : 0 ÷ 2.6 / 2nd : 0 ÷ 4.0","1st : 0 ÷ 2.6 / 2nd : 0 ÷ 4.3","1st : 0 ÷ 2.7 / 2nd : 0 ÷ 4.3","1st : 0 ÷ 2.6 / 2nd : 0 ÷ 4.5","1st : 0 ÷ 2.6 / 2nd : 0 ÷ 4.5","1st : 0 ÷ 2.6 / 2nd : 0 ÷ 4.5","1st : 0 ÷ 2.6 / 2nd : 0 ÷ 4.5","1st : 0 ÷ 2.5 / 2nd : 0 ÷ 4.5","1st : 0 ÷ 2.3 / 2nd : 0 ÷ 4.5","1st : 0 ÷ 2.3 / 2nd : 0 ÷ 4.5"]
["Slew speed (rpm) ",10.5,11,11,9.5,10.5,10.5,10.5,10.5,10,10,10.5,10.5,10.5,9.5,9.5,11,11,11]
["CONTROLS"]
["Boom, dipper stick, bucket and turret swing ","2 pilot joysticks","2 pilot joysticks","2 pilot joysticks","2 electro-proportional joysticks","2 pilot joysticks","2 pilot joysticks","2 pilot joysticks","2 pilot joysticks","2 electro-proportional joysticks","2 pilot joysticks","2 pilot joysticks","2 pilot joysticks","2 pilot joysticks","2 pilot joysticks","2 pilot joysticks","2 pilot joysticks","2 pilot joysticks","2 pilot joysticks"]
["Positioner two pieces boom ","-","-","-","-","-","-","electroproportional switch on right joystick","-","-","-","-","-","-","-","-","-","-","-"]
["Track movements (included counter rotation) ","2 pilot levers","2 pilot levers","2 pilot levers","2 electro-proportional levers","2 mechanical levers","2 mechanical levers","2 pilot levers","2 pilot levers","2 electro-proportional levers","2 pilot levers","2 pilot levers","2 pilot levers","2 pilot levers","2 pilot levers","2 pilot levers","2 pilot levers","2 pilot levers","2 pilot levers"]
["Dozer blade ","pilot lever","pilot lever","pilot lever","electro-proportional lever","pilot lever","pilot lever","pilot lever","pilot lever","electro-proportional lever","pilot lever","pilot lever","pilot lever","pilot lever","pilot lever","pilot lever","pilot lever","pilot lever","pilot lever"]
["Auxiliary system - AUX 1 ","electroproportional switch on right joystick","electroproportional switch on right joystick*","electroproportional switch on right joystick*","electroproportional\nswitch on joystick","right pedal","right pedal","electroproportional switch on right joystick","electroproportional switch on right joystick**","electroproportional switch on joystick","electroproportional switch on right joystick*","electroproportionalswitch on right joystick**","electroproportionalswitch on right joystick**","electroproportionalswitch on right joystick**","electroproportionalswitch on right joystick**","electroproportionalswitch on right joystick**","electroproportional\nswitch on right joystick**","electroproportionalswitch on right joystick**","electroproportional\nswitch on right joystick**"]
["Auxiliary system - AUX 2 ","-","-","-","electroproportional\nswitch on joystick","-","-","-","-","electroproportional switch on joystick","-","electroproportional\nswitch on left joystick\nelectroproportional","electroproportional switch on right joystick","electroproportional switch on right joystick","electroproportional switch on right joystick","electroproportional switch on right joystick","-","electroproportional switch on right joystick","electroproportional switch on right joystick"]
["Auxiliary system - AUX 3 ","-","-","-","electroproportional\nswitch on joystick","-","-","-","-","electroproportional switch on joystick","-","-","electroproportional switch on left joystick","electroproportional switch on left joystick","electroproportional\nswitch on left joystick","electroproportional switch on left joystick","-","electroproportional\nswitch on left joystick","electroproportional\nswitch on left joystick"]
["Boom swing ","electroproportional switch on left joystick","electroproportional switch on left joystick","electroproportional switch on left joystick","electroproportional switch on left joystick","left pedal","left pedal","electroproportional switch on left joystick","electroproportional switch on left joystick","Boom swing electroproportional switch on left joystick","electroproportional switch on left joystick","electroproportional switch on left joystick","electroproportional switch on left joystick","electroproportional switch on left joystick","electroproportional switch on left joystick","electroproportional switch on left joystick","electroproportional\nswitch on left joystick","electroproportional switch on left joystick","electroproportional switch on left joystick"]
["WEIGHTS"]
["Transport weight with roll-bar (with FOPS 1 roof) kg ","-","1200 (1225)***","1255 (1280)***","1315***","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["Operating weight with roll-bar (with FOPS 1 roof) ISO 6016 kg ","-","1305 (1330)***","1360 (1385)***","1420***","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
["Transport weight with canopy kg ","1770***","-","-","-","1580***","1720***","1900***","2090***","2210***","2450***","-","-","-","-","-","-","-","-"]
["Transport weight with cab kg ","1880***","-","-","-","1690***","1830***","2010***","2190***","2340***","2580***","3330***","4200***","4600***","4800***","5250***","5440***","5740***","6290***"]
["Operating weight with canopy ISO 6016 kg ","1880***","-","-","-","1690***","1830***","2010***","2220***","2340***","2580***","-","-","-","-","-","-","-","-"]
["Operating weight with cab ISO 6016 kg ","1990***","-","-","-","1800***","1940***","2120***","2320***","2470***","2710***","3480***","4350***","4750***","4950***","5400***","5670***","5970***","6520***"]
["CIRCUIT AND COMPONENT CAPACITIES"]
["Fuel tank (l) ",25,14.5,14.5,"-",25,25,25,20,"-",26,49,60,60,75,75,85,85,85]
["Hydraulic oil tank (l) ",20,9.5,9.5,"-",20,20,20,16,"-",29,33.5,50,50,65,65,60,60,60]
["Hydraulic circuit capacity (l) ",29,15,15,"-",29,29,30,25,"-",40,54,65,65,85,85,80,80,80]
["Cooling system capacity (l) ",4.5,4.3,4.3,"-",4.5,4.5,4.5,4,"-",5,7.5,9,9,11,11,12,12,12]
["Engine oil (l) ",2.8,3.8,3.8,"-",2.4,2.4,2.8,4.4,"-",2.8,6.3,7,7,10.6,10.6,10.2,10.2,10.2]
["SUPPLY"]
["Battery chemistry ","-","-","-","lithium-ion","-","-","-","-","lithium-ion","-","-","-","-","-","-","-","-","-"]
["Gross capacity (kWh) ","-","-","-",21.5,"-","-","-","-",32.3,"-","-","-","-","-","-","-","-","-"]
["Nominal voltage of the system (V) ","-","-","-",102,"-","-","-","-",102,"-","-","-","-","-","-","-","-","-"]
["Autonomy according to the operating mode (h) ","-","-","-","4 ÷ 8","-","-","-","-","4 ÷ 8","-","-","-","-","-","-","-","-","-"]
["CHARGING TIMES"]
["On-board charger 220V (h) ","-","-","-",10,"-","-","-","-",9,"-","-","-","-","-","-","-","-","-"]
["External three-phase rapid charge 380V (Optional) (h) ","-","-","-","1,0 (80%) - 1,5 (100%)","-","-","-","-","1.5 (80%) - 2.0 (100%)","-","-","-","-","-","-","-","-","-"]
["OPERATING MODES"]
["Type ","-","-","-","ECO/ STD/ PWR","-","-","-","-","ECO/ STD/ PWR","-","-","-","-","-","-","-","-","-"]
["Max. rpm ","-","-","-","2400/ 2600/ 2800","-","-","-","-","2400/ 2600/ 2800","-","-","-","-","-","-","-","-","-"]
["* with latch\n** with holding function\n*** with rubber tracks"]