{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":43,"n_cols":5,"rows_kept":43,"cut":false,"hidden":false,"merged":[[42,0,42,6]]}
[]
[null,"TR270B","TR310B","TV370B","TV450B"]
["DIMENSIONI GENERALI"]
["Altezza al perno benna mm ",3178,3178,3343,3344]
["Altezza alla sommità ROPS mm ",1998,1998,2044,2044]
["Lunghezza senza attrezzo mm ",2662,2662,2984,3050]
["Lunghezza con benna DF (con benna LPE) * mm ","3280 (3512)","3280 (3512)","3604 (3835)","3667 (3899)"]
["Larghezza fuori tutto mm ",1676,1887,1943,1943]
["Passo mm ","-","-","-","-"]
["Luce libera da terra mm ",207,207,244,244]
["Altezza di scarico con benna DF (con benna LPE) * mm ","2556 (2410)","2556 (2410)","2669 (2505)","2645 (2481)"]
["Angolo di scarico °  ",38,38,53,45]
["Sbraccio di scarico all’altezza max con benna DF (con benna LPE)* mm ","566 (745)","566 (745)","716 (880)","727 (891)"]
["Angolo di rampa ° ",32,32,32,32]
["Angolo di richiamo (benna a terra) ° ",31,31,35,32]
["SPECIFICHE"]
["Dimensioni telaio ","Medio","Medio","Grande","Grande"]
["Livello di emissioni ","Stage V","Stage V","Stage V","Stage V"]
["DATI PRESTAZIONALI"]
["Capacità operativa nominale 50% kg ","50%: 1225 35%: 860","50%: 1406 35%: 984","50%: 1682 35%: 1178","50%: 2045 35%: 1432"]
["ROC senza contrappesi 50% kg ","50%: 1280 35%: 915","50%: 1461 35%: 1039","50%: 1927 35%: 1331","50%: 2343 35%: 1618"]
["Carico di ribaltamento kg ",2450,2810,3364,4091]
["Forza di strappo al cilindro di sollevamento** kN ","27,8","29,0","26,8","33,9"]
["Forza di strappo al cilindro benna** kN ","32,3","38,6","33,4","41,8"]
["MOTORE"]
["Marca e modello del motore ","FPT F5H","FPT F5H","FPT F5H","FPT F5M"]
["Cilindrata l ","2025-03-04","2025-03-04","2025-03-04","2025-03-06"]
["Potenza hp (kW)/rpm ","74 (55)@ 2500","74 (55)@ 2500","74 (55) @ 2500","90 (67)@ 2500"]
["Coppia max. Nm/rpm ","314 @ 1400","314 @ 1400","314 @ 1400","383 @ 1400"]
["VELOCITÀ DI TRASLAZIONE"]
["Bassa velocità km/h ","2025-08-09","2025-08-09","2025-08-09","2025-08-09"]
["Alta velocità (optional) km/h ","2025-12-09","2025-12-09","2025-12-09","2025-12-09"]
["IMPIANTO IDRAULICO"]
["Portata pompa LPM ",92,92,92,92]
["Alta portata optional LPM ",123,123,143,149]
["Pressione di scarico bar ",210,210,210,210]
["“Enhanced High Flow” opzionale bar ","-","-","-",276]
["PESI"]
["Peso operativo kg ",3750,4027,4370,4823]
["Peso alla spedizione kg ",3615,3891,4220,4667]
["RIFORNIMENTI"]
["Serbatoio carburante l ","73,8","73,8","96,5","96,5"]
["* Con benna standard** Forze di strappo stimate considerando sia il ribaltamento che i limiti idraulici."]