{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":74,"n_cols":9,"rows_kept":74,"cut":false,"hidden":false,"merged":[]}
[]
[null,"721G ","521G ","621G ","651G ","821G ","921G ","1021G ","1121G "]
["ENGINE"]
["Maker & Model ","FPT N67","FTP N45","FTP N67","FTP N67","FPT N67","FPT N67","FTP Cursor 9","FTP Cursor 9"]
["No. of cylinders ",6,4,6,6,6,6,6,6]
["Displacement (l) ",6.7,4.5,6.7,6.7,6.7,6.7,8.7,8.7]
["Air intake ","Turbocharger with air-to-air cooling. No EGR valve is used:\nOnly fresh air is taken for combustion and no extra cooling system is needed.","Turbocharger with air-to-air cooling. No EGR valve is used:\nOnly fresh air is taken for combustion and no extra cooling system is needed.","Turbocharger with air-to-air cooling. No EGR valve is used:\nOnly fresh air is taken for combustion and no extra cooling system is needed.","Turbocharger with air-to-air cooling. No EGR valve is used:\nOnly fresh air is taken for combustion and no extra cooling system is needed.","Turbocharger with air-to-air cooling. No EGR valve is used:\nOnly fresh air is taken for combustion and no extra cooling system is needed.","Turbocharger with air-to-air cooling. No EGR valve is used:\nOnly fresh air is taken for combustion and no extra cooling system is needed.","Turbocharger with air-to-air cooling. No EGR valve is used: Only fresh air is taken for\ncombustion and no extra cooling system is needed.","Turbocharger with air-to-air cooling. No EGR valve is used: Only fresh air is taken for\ncombustion and no extra cooling system is needed."]
["Injection ","Common Rail Multiple Injection.","Common Rail Multiple Injection.","Common Rail Multiple Injection.","Common Rail Multiple Injection.","Common Rail Multiple Injection.","Common Rail Multiple Injection.","Common Rail Multiple Injection.","Common Rail Multiple Injection."]
["After Treatment System ","HI-eSCR 2 (DOC+SCRoF)","HI-eSCR 2 (DOC+SCRoF)","HI-eSCR 2 (DOC+SCRoF)","HI-eSCR 2 (DOC+SCRoF)","HI-eSCR 2 (DOC+SCRoF)","HI-eSCR 2 (DOC+SCRoF)","HI-eSCR 2 (DOC+SCRoF)","HI-eSCR 2 (DOC+SCRoF)"]
["Emission level ","Compliant with EU Stage V","Compliant with EU Stage V","Compliant with EU Stage V","Compliant with EU Stage V","Compliant with EU Stage V","Compliant with EU Stage V","Compliant with EU Stage V","Compliant with EU Stage V"]
["Maximum power (Peak Gross-Peak Net) (kW/hp) ","145/195","106/142 - 99/133","128/172 - 121/162","128/172 - 121/162","172/230","190/255","239/320","250/347"]
["@ Engine speed (ISO 14396) (rpm) ",2000,1800,1800,1800,1800,1600,1800,1800]
["Maximum Torque (Gross-Net) (Nm) ",950,"612/586","730/692","730/692",1184,1300,1479,1604]
["TRANSMISSION"]
["ProShift ","5-speed powershift with lock up (optional). Lock up clutch eliminates torque converter losses from second gear up to fifth gear.\nIntelligent Clutch Cut Off (ICCO) with Power Inch: Proportional declutching.","-","5-speed powershift with lock up (optional). Lock up clutch eliminates torque converter losses from second gear up to fifth gear.\nIntelligent Clutch Cut Off (ICCO) with Power Inch: Proportional declutching.","5-speed powershift with lock up (optional). Lock up clutch eliminates torque converter losses from second gear up to fifth gear.\nIntelligent Clutch Cut Off (ICCO) with Power Inch: Proportional declutching.","5-speed powershift with lock up (optional). Lock up clutch eliminates torque converter losses from second gear up to fifth gear.\nIntelligent Clutch Cut Off (ICCO) with Power Inch: Proportional declutching.","5-speed powershift with lock up (optional). Lock up clutch eliminates torque converter losses from second gear up to fifth gear.\nIntelligent Clutch Cut Off (ICCO) with Power Inch: Proportional declutching.","-","-"]
["Forward 1 (km/h) ",7,"-",7,7,7,6,"-","-"]
["Forward 2 (km/h) ",13,"-",13,13,11,11,"-","-"]
["Forward 3 (km/h) ",19,"-",20,20,17,17,"-","-"]
["Forward 4 (km/h) ",30,"-",31,31,26,26,"-","-"]
["Forward 5 (km/h) ",40,"-",45,45,40,40,"-","-"]
["Reverse 1 (km/h) ",8,"-",7,7,7,7,"-","-"]
["Reverse 2 (km/h) ",14,"-",14,14,12,12,"-","-"]
["Reverse 3 (km/h) ",31,"-",32,32,28,28,"-","-"]
["4-speed ZF Powershift ","with Intelligent Clutch Cut Off (ICCO)","with Intelligent Clutch Cut Off (ICCO)","with Intelligent Clutch Cut Off (ICCO)","with Intelligent Clutch Cut Off (ICCO)","with Intelligent Clutch Cut Off (ICCO)","with Intelligent Clutch Cut Off (ICCO)","with Intelligent Clutch Cut Off (ICCO)","with Intelligent Clutch Cut Off (ICCO)"]
["Forward 1 (km/h)  ",8,6,7,7,7,7,7,7]
["Forward 2 (km/h)  ",13,11,13,13,12,12,13,12]
["Forward 3 (km/h)  ",25,22,24,24,23,23,19,18]
["Forward 4 (km/h)  ",37,36,39,39,37,36,38,38]
["Reverse 1 (km/h)  ",8,6,7,7,7,7,7,7]
["Reverse 2 (km/h)  ",13,12,14,14,13,13,13,13]
["Reverse 3 (km/h)  ",26,23,25,25,25,25,27,25]
["AXLES (available options)"]
["Heavy Duty ZF Axles with Limited Slip Differential on both front and rear axle ","yes","-","yes","yes","yes","-","-","-"]
["Heavy Duty ZF Axles with automatic 100% differential lock on front and open ","yes","yes","yes","yes","yes","yes","yes","yes"]
["Heavy Duty ZF Axles with automatic 100% differential lock on front and LSD on rear axle ","yes","-","yes","yes","yes","-","yes","yes"]
["Standard ZF Axles with Limited Slip Differential on both front and rear axle ","-","yes","yes","-","-","-","-","-"]
["Axles oscillation angle (total) (°) ",24,24,24,24,24,24,"24°","24°"]
["TIRES"]
["Standard tire’s size ","20.5R25","17.5R25","20.5R25","20.5R25","23.5R25","23.5R25","26.5R25","26.5R25"]
["BRAKES"]
["Service brake ","Maintenance free, self-adjusting wet 4-wheel disc brakes.","Maintenance free, self-adjusting wet 4-wheel disc brakes.","Maintenance free, self-adjusting wet 4-wheel disc brakes.","Maintenance free, self-adjusting wet 4-wheel disc brakes.","Maintenance free, self-adjusting wet 4-wheel disc brakes.","Maintenance free, self-adjusting wet 4-wheel disc brakes.","Maintenance free, self-adjusting wet 4-wheel disc brakes.","Maintenance free, self-adjusting wet 4-wheel disc brakes."]
["Service brake disc area (m²/hub) ",0.39,0.31,0.39,0.39,0.39,0.47,0.74,0.74]
["Parking brake ","With the negative brake all four wheels are automatically stopped when the engine is stopped.","With the negative brake all four wheels are automatically stopped when the engine is stopped.","With the negative brake all four wheels are automatically stopped when the engine is stopped.","With the negative brake all four wheels are automatically stopped when the engine is stopped.","With the negative brake all four wheels are automatically stopped when the engine is stopped.","With the negative brake all four wheels are automatically stopped when the engine is stopped.","With the negative brake all four wheels are automatically stopped\nwhen the engine is stopped.","With the negative brake all four wheels are automatically stopped\nwhen the engine is stopped."]
["Parking brake disc area(cm²) ",82,58,58,58,82,82,82,82]
["HYDRAULICS"]
["Loader control valve ","Bosch-Rexroth, closed centre, load sensing/flow sharing.","Bosch-Rexroth, closed centre, load sensing/flow sharing.","Bosch-Rexroth, closed centre, load sensing/flow sharing.","Bosch-Rexroth, closed centre, load sensing/flow sharing.","Bosch-Rexroth, closed centre, load sensing/flow sharing.","Bosch-Rexroth, closed centre, load sensing/flow sharing.","Bosch-Rexroth, closed centre, load sensing/flow sharing. 3 spool main control valve.","Bosch-Rexroth, closed centre, load sensing/flow sharing. 3 spool main control valve."]
["Steering ","Steering cylinders actuated by hydraulic orbitrol under priority valve, controlled, in turn,\nby active load sensing signal.","Steering cylinders actuated by hydraulic orbitrol under priority valve, controlled, in turn,\nby active load sensing signal.","Steering cylinders actuated by hydraulic orbitrol under priority valve, controlled, in turn,\nby active load sensing signal.","Steering cylinders actuated by hydraulic orbitrol under priority valve, controlled, in turn,\nby active load sensing signal.","Steering cylinders actuated by hydraulic orbitrol under priority valve, controlled, in turn,\nby active load sensing signal.","Steering cylinders actuated by hydraulic orbitrol under priority valve, controlled, in turn,\nby active load sensing signal.","Steering cylinders actuated by hydraulic orbitrol under priority valve, controlled,\nin turn, by active load sensing signal.","Bosch-Rexroth, closed centre, load sensing/flow sharing. 3 spool main control valve."]
["Loader controls ","Pilot with proportional solenoid valves controlled by\nelectro-hydraulic single joystick or single-axis 2/3 levers.","Pilot with proportional solenoid valves controlled by\nelectro-hydraulic single joystick or single-axis 2/3 levers.","Pilot with proportional solenoid valves controlled by\nelectro-hydraulic single joystick or single-axis 2/3 levers.","Pilot with proportional solenoid valves controlled by\nelectro-hydraulic single joystick or single-axis 2/3 levers.","Pilot with proportional solenoid valves controlled by\nelectro-hydraulic single joystick or single-axis 2/3 levers.","Pilot with proportional solenoid valves controlled by\nelectro-hydraulic single joystick or single-axis 2/3 levers.","Pilot with proportional solenoid valves controlled by electro-hydraulic\nsingle joystick or single-axis 2/3 levers.","Pilot with proportional solenoid valves controlled by electro-hydraulic\nsingle joystick or single-axis 2/3 levers."]
["Pump type ","Single, variable displacement","Single, variable displacement","Single, variable displacement","Single, variable displacement","Tandem, variable displacement","Tandem, variable displacement","Tandem, variable displacement","Tandem, variable displacement"]
["Max oil flow (l/min) ",206,134,169,190,236,278,348,376]
["@ engine speed (rpm) ",2000,2000,2000,2000,2000,2000,2000,2000]
["AUXILIARY HYDRAULICS"]
["Max oil flow (l/min) ",206,134,169,188,236,278,240,240]
["Max pressure (bar) ","249-255","249-255","249-255","249-255","249-255","249-255","249-255","249-255"]
["FLUIDS CAPACITIES"]
["Fuel tank, usable volume (l) ",246,189,248,248,288,288,459,459]
["DEF (AdBlue®) tank (l) ",41.3,41.3,41.3,41.3,41.3,41.3,65,65]
["Engine coolant (l) ",28,22,27,27,30,30,57,57]
["Engine oil (l) ",13,12,13,13,13,13,26,26]
["Hydraulic oil tank (l) ",91,57,91,91,91,91,134,134]
["Total hydraulic system oil (l) ",180,114,148,148,180,200,250,250]
["Front and Rear Axles (l) ","35+35","22+22","22+22","22+22","40+40","42+40","68+68","68+68"]
["Transmission oil (l) ",34,19,27,27,34,34,45,45]
["CAB PROTECTION"]
["Protection against falling objects (FOPS) ","According to ISO EN 3449 std.","According to ISO EN 3449 std.","According to ISO EN 3449 std.","According to ISO EN 3449 std.","According to ISO EN 3449 std.","According to ISO EN 3449 std.","According to ISO EN 3449 std.","According to ISO EN 3449 std."]
["Protection against roll-over (ROPS) ","According to ISO EN 13510 std.","According to ISO EN 13510 std.","According to ISO EN 13510 std.","According to ISO EN 13510 std.","According to ISO EN 13510 std.","According to ISO EN 13510 std.","According to ISO EN 13510 std.","According to ISO EN 13510 std."]
["NOISE AND VIBRATION"]
["In the cab - LpA (dB) (ISO 6396-2008) ",68,68,68,68,68,69,68,69]
["Outside - LwA (dB) (2000/14/EC) ",103,102,104,104,104,104,105,104]
["Vibrations ","Operator’s seat meets the criteria of ISO 7096:2000.\nThe vibrations transmitted do not exceed 0.5 m/s²","Operator’s seat meets the criteria of ISO 7096:2000.\nThe vibrations transmitted do not exceed 0.5 m/s²","Operator’s seat meets the criteria of ISO 7096:2000.\nThe vibrations transmitted do not exceed 0.5 m/s²","Operator’s seat meets the criteria of ISO 7096:2000.\nThe vibrations transmitted do not exceed 0.5 m/s²","Operator’s seat meets the criteria of ISO 7096:2000.\nThe vibrations transmitted do not exceed 0.5 m/s²","Operator’s seat meets the criteria of ISO 7096:2000.\nThe vibrations transmitted do not exceed 0.5 m/s²","Operator’s seat meets the criteria of ISO 7096:2000.\nThe vibrations transmitted do not exceed 0.5 m/s²","Operator’s seat meets the criteria of ISO 7096:2000.\nThe vibrations transmitted do not exceed 0.5 m/s²"]
["ELECTRICAL SYSTEM"]
["System voltage (V) ",24,24,24,24,24,24,24,24]
["Batteries (n° x V) ","2 x 12","2 x 12","2 x 12","2 x 12","2 x 12","2 x 12","2 x 12","2 x 12"]
["Alternator - capacity (A) ",120,70,120,120,120,120,120,120]