{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":42,"n_cols":10,"rows_kept":42,"cut":false,"hidden":false,"merged":[[41,0,41,11]]}
[]
[null,"SR200B","SR130B","SR150B","SR175B","SV185B","SR220B","SR250B","SV250B","SV300B"]
["GENERAL DIMENSIONS"]
["Overall Height w/ LPE Bkt mm ",4146,3859,3859,4121,4055,4198,4198,4304,4304]
["Bucket Hinge Pin mm ",3124,2845,2845,3099,3048,3178,3178,3302,3302]
["Top Of ROPS mm ",1998,1919,1919,1974,1974,2002,2002,2002,2002]
["Bottom of Bkt Fully Raised mm ",2950,2682,2682,2925,2877,2998,2998,3038,3038]
["Length w/o Attachment mm ",2669,2435,2435,2685,2685,2981,2981,2990,2990]
["Length w/ LPE Bkt mm ",3525,3297,3297,3538,3578,3843,3843,3835,3835]
["Dump Angle ° ",39.6,40.2,40.2,39.6,51.9,38.1,38.1,53.5,53.5]
["Dump Height w/ LPE Bkt mm ","2347 @ 39.6°","2073 @ 40.2°","2073 @ 40.2°","2322 @ 39.6°","2214 @ 45°","2419 @ 39.6°","2419 @ 39.6°","2465 @ 45°","2465 @ 45°"]
["Dump Reach w/ LPE Bkt mm ","696 @ 39.6°","675 @ 40.2°","675 @ 40.2°","721 @ 39.6°","946 @ 45°","677 @ 39.6°","677 @ 39.6°","837 @ 45°","837 @ 45°"]
["Max Rollback at Ground ° ",31,26.12,26.12,31.6,35,30.7,30.7,35,35]
["Max Rollback Fully Raised ° ",98.6,95.2,95.2,98.6,87.6,99.7,99.7,86,86]
["Wheelbase mm ",1128,941,941,1128,1128,1322,1322,1322,1322]
["Ground Clearance mm ",203,178,178,178,178,203,203,203,203]
["Angle of Departure ° ",25,22,22,23,23,23.5,23.5,23.5,23.5]
["Rear Axle to Bumper mm ",924,858,858,924,924,1034,1034,1034,1034]
["Overall Width (Spec Tire) mm ",1755,1518,1518,1642,1642,1768,1768,1768,1768]
["PERFORMANCE SPECS"]
["Rated Operating Capacity 50% kg ",905,590,680,790,840,1000,1135,1135,1364]
["Tipping Load kg ",1814,1179,1361,1588,1678,2000,2270,2270,2727]
["Lift Cylinder Breakout Force* kN ",20.3,12.7,14.1,16.9,15.3,24.4,25.3,21.4,25.5]
["Bucket Cylinder Breakout Force* kN ",32.3,18.6,18.6,32.3,24.7,38.7,33.3,33.7,33.7]
["ENGINE"]
["Engine Brand ","FPT","PERKINS","PERKINS","PERKINS","PERKINS","FPT","FPT","FPT","FPT"]
["Engine Model ","F5C E5454 G*A001","404D-22","404D-22T","404D-22T","404D-22T","F5C E5454 B*A005","F5C E5454 C*A003","F5C E5454 B*A005","F5C E5454 C*A003"]
["Displacement l ",3.2,2.2,2.2,2.2,2.2,3.2,3.2,3.2,3.2]
["Horsepower Gross kW ","55 @ 2500","36.4 @ 2800","44.7 @ 2800","44.7 @ 2800","44.7 @ 2900","61 @ 2500","67 @ 2500","61 @ 2500","67 @ 2500"]
["Peak torque N·m ","275 @ 1400","143 @ 1800","171 @ 1800","171 @ 1800","171 @ 1800","305 @ 1400","340 @ 1400","305 @ 1400","340 @ 1400"]
["TRAVEL SPEED"]
["Low Range Km/h ",10.9,12.7,12.7,12.7,12.7,11.3,11.3,11.3,11.3]
["High Range (Optional) Km/h ",15.9,18,18,18,18,16.9,16.9,16.9,16.9]
["HYDRAULIC SYSTEM"]
["Pump flow 100% Lpm ",85,59,59,72,72,85,85,85,85]
["Displacement cc ",34.1,20.4,20.4,24.9,24,34.1,34.1,34.1,34.1]
["WEIGHTS"]
["Operating Weight kg ",3184,2344,2474,2881,3019,3436,3547,3687,3822]
["Shipping Weight kg ",3025,2160,2300,2705,2840,3200,3340,3475,3610]
["SERVICE CAPACITY"]
["Fuel Tank l ",75.7,60.5,60.5,75.7,75.7,96.5,96.5,96.5,96.5]
["* Breakout forces estimated considering both tip and hydraulic limits"]