{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":52,"n_cols":3,"rows_kept":52,"cut":false,"hidden":false,"merged":[]}
[]
[null,"450 DX","752 EX"]
["ENGINE"]
["Engine Model ","MDI - 2500","S8000"]
["Engine Make ","Mahindra & Mahindra","FPT"]
["Max. Gross Power ","33.6 kW/ 45 HP @2300 rpm (ISO 14396)","76 HP @2200 rpm"]
["Type ","4-Cylinder","4-Cylinder, Inline, 4 Stoke, Turbo Charged, Water Cooled"]
["Displacement ","2523 L","3908 cc"]
["Bore x Stroke ","-","104x115 mm"]
["Starting Method ","-","12 V, Electrical system"]
["Propulsion on front and rear drum ","-","Hydrostatic drive"]
["POWER TRAIN"]
["Working Speed ","12 km/hr","0-5.5 Kmph"]
["Travel Speed ","12 km/hr","0-11 Kmph"]
["Gradeability with/without vibration (%) ","25/30","-"]
["STEERING"]
["Steering ","Hydrostatic (Center Point Articulation)","-"]
["Steering Angle (°) ","±33","-"]
["Turning radius (m) ",3,"-"]
["Oscillation angle (°) ","±10","-"]
["BRAKES"]
["Service Brake ","Hydrostatic","Hydrostatic"]
["Parking Brake ","Spring applied, hydraulically released on rear drum","Hydraulic"]
["OPERATION DATA"]
["Operating Weight (kg) ",3225,9061]
["Front Axle Load (kg) ",1550,4470]
["Rear Axle Load (kg) ",1675,4591]
["Static Linear Load - Front (kg/cm) ",13.4,"26. 7"]
["Static Linear Load - Rear (kg/cm) ","-",27.4]
["Gradeability (% (20)°) ","-",36]
["Articulation to either side (°) ","-",25]
["Inside Turning Radius (mm) ","-",5.8]
["Oscillation Angle (°) ","-",10]
["Vibration Stage ","-","Two"]
["Nominal Amplitude (Stage 1) (mm) ",0.6,1]
["Nominal Amplitude (Stage 2) (mm) ","-",0.4]
["Frequency (Stage 1) (Hz) ",65,33.3]
["Frequency (Stage 2) (Hz) ",55,50]
["SERVICE CAPACITIES"]
["Water Tank Capacity (L) ",110,390]
["Fuel Tank Capacity (L) ",45,140]
["Hydraulic Tank Capacity (L) ",45,80]
["Water spray nozzles ","6 Nozzles per drum","-"]
["Water tank material ","Plastic","-"]
["VIBRATION SYSTEM"]
["Vibration Stage ","Two","-"]
["Frequency High - HF (Hz) ",65,"-"]
["Frequency Low - LF (Hz) ",55,"-"]
["Amplitude (mm) ",0.6,"-"]
["Centrifugal Force (High) - per drum (kgf/kN) ","4360 / 42.76","-"]
["Centrifugal Force (Low) - per drum (kgf/kN) ","3120 / 30.66","-"]
["Maximum Applied Force - per drum (kgf/kN) ","6035 /59.18","-"]