{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":45,"n_cols":8,"rows_kept":45,"cut":false,"hidden":false,"merged":[]}
[]
[null,"921F","621XS","621F","721F","821F","1021F","1121F"]
["PRODUCTIVITY (50 meter distance cycle)"]
["Considering density at 1,8 t/m³ and 100% fill factor 52 cycles/hour including 5 minute break ","210 m³/h or 375 t/h 52 loading cycles/h with standard bucket 4.0 m³ or 7.2 ton","-","52 loading cycles/h with 2.4 m³ bucket 125 m³/h or 225 t/h of material","140 m³/h or 280 t/h 52 loading cycles/h with standard bucket 2.7 m³ or 5.4 ton","160 m³/h or 320 t/h 52 loading cycles/h with standard bucket 3.4 m³ or 6.2 ton","230 m³/h or 410 t/h 52 loading cycles/h with standard bucket 4.4 m³ or 7.9 ton","260 m³/h or 460 t/h 52 loading cycles/h with standard bucket 5.0 m³ or 8.8 ton"]
["ENGINE"]
["Make ","FPT turbocharged engine F4HFA613D with  Tier 2 (EU stage II regulations)","FPT , NEF 6 Tier 3 , Turbocharger intercooler","FPT engine F4HFA613F compliant with with EPA  Tier3 or EU Stage 3A regulations","FPT turbocharged engine F4HE9684F*J with Tier 3 (EU stage 3a)","FPT turbocharged engine F4HE9684E*J with Tier 3 (EU stage 3a )","FPT turbocharged engine F2CFA614C-E019 with Tier 2 (EU stage II regulations)","FPT turbocharged engine F2CFA614B*E019 with Tier 2 (EU stage II regulations)"]
["Cylinders ",6,6,6,6,6,6,6]
["Max power SAE J1995 ","190kW / 255 hp @1800 rpm","97 kW/ 130 hp @2350 rpm","128 kW / 172 hp @1800 rpm","145 kW / 195 hp @2000 rpm","172 kW / 230 hp @1800 rpm","239 kW / 320 hp @1800 rpm","259 kW / 347 hp @1800 rpm"]
["Maximum torque SAE J995 ","1300 Nm @1300 rpm","443 Nm @1500 rpm","730 Nm @1600 rpm","862 Nm @1400 rpm","1002 Nm @ 1500 rpm","1479 Nm @1100 rpm","1604 Nm @1100 rpm"]
["TRANSMISSION"]
["Forward speeds ","7-12-23-36 Km/h","6.4-11.6-22.3-36.2 Km/h","7-13-24-39 Km/h","8-13-25-37 Km/h","7-12-23-37 Km/h","7-13-19-38 Km/h","7-12-18-38 Km/h"]
["Reverse speeds ","7-13-24 Km/h","6.7-12.2-23.8 Km/h","7-14-25 Km/h","8-13-26 Km/h","7-13-25 Km/h","7-13-27 Km/h","7-13-26 Km/h"]
["AXLES AND DIFFERENTIAL"]
["Limited slip differential front and rear ","-","Standard","29% Limited slip differential on front and rear axles","when one wheel slips 73% of the available axle torque is guaranted on the other wheel","when one wheel slips 73% of the available axle torque is guaranted on the other wheel","-","-"]
["Front ","ZF Heavy Duty axles with 100% front auto-lock differential","ZF","Heavy duty axle type MT-L3075-II - dynamic load: 12.700kg","Heavy Duty axle +(ZF type MT-L3085-II)","Heavy Duty axle +(ZF type MT-L3095-II)","ZF type MT-L3115-II","Heavy Duty (ZF type MT-L3115-II)"]
["Rear ","ZF Heavy Duty axles with 100% front auto-lock differential","ZF","ZF type MT-3065-II - dynamic load 10.700kg","standard axle (ZF type MT-L3075-II)","standard axle (ZF type MT-L3085-II)","ZF type MT-L3105-II","Heavy Duty (ZF type MT-L3115-II)"]
["Rear axle total oscillation ","24°","-","24°","24°","24°","26°","26°"]
["TYRES"]
["Tyres ","23.5R25","17.5 x 25 12 Ply L2 or 16 Ply L3","20.5R25","20.5R25","23.5R25","26.5R25","26.5R25"]
["BRAKES"]
["Service brake ","Maintenance free, self-adjusting wet 4-wheel disc brakes","-","Maintenance free, self-adjusting wet 4-wheel disc brakes","Maintenance free, self-adjusting wet 4-wheel disc brakes","Maintenance free, self-adjusting wet 4-wheel disc brakes","Maintenance free, self-adjusting wet 4-wheel disc brakes","Maintenance free, self-adjusting wet 4-wheel disc brakes"]
["Area ","0.47 m²/hub","-","0,39 m²/hub","0,39 m²/hub","0,39 m²/hub","0.74 m²/hub (L3115-II axle) or 0.54 m²/hub (L3105-II axle)","0.74 m²/hub"]
["Parking brake ","Disc brake on transmission activated from the cab cluster","-","Disc brake on transmission activated from the cab cluster","Disc brake on transmission activated from the cab cluster","Disc brake on transmission activated from the cab cluster","Disc brake on transmission activated from the cab cluster","Disc brake on transmission activated from the cab cluster"]
["HYDRAULICS"]
["Valves ","Rexroth Closed-center, Load sensing hydraulic system. Main valve with 3 sections","Open centre , Positive Low Pressure","Rexroth Closed-center, Load sensing hydraulic. Main valve with 3 sections","Rexroth Closed-center, Load sensing hydraulic system. Main valve with 3 sections","Rexroth Closed-center, Load sensing hydraulic system. Main valve with 3 sections","Rexroth Closed-center, load sensing hydraulic system Main valve with 3 sections","Rexroth Closed-center, load sensing hydraulic system Main valve with 3 sections"]
["Steering ","The steering orbitrol is hydraulically actuated with priority valve","-","The steering orbitrol hydraulically is actuated with priority valve","The steering orbitrol hydraulically  is actuated with priority valve","The steering orbitrol hydraulically is actuated  with priority valve","The steering orbitrol hydraulically is actuated with priority valve","The steering orbitrol hydraulically  is actuated with priority valve"]
["Type of pump ","Tandem Variable displacement pump (282 l/min @2000 rpm)","Dual Gear Pump (140 l/min)","Tandem Variable displacement pump (171 l/min @250 bar)","Tandem Variable displacement pump (206 l/min @2000 rpm)","Tandem Variable displacement pump (240 l/min @2000 rpm)","Tandem Variable displacement pump  (352 l/min @2000 rpm)","Tandem Variable displacement pump (380 l/min @2000 rpm)"]
["Control type ","Pilot control with single joystick or two levers","-","Pilot control with single joystick or two levers","Pilot control with single joystick or two levers","Pilot control with single joystick or two levers","Pilot control with single joystick or two levers","Pilot control with single joystick or two levers"]
["CAPACITIES"]
["Fuel tank ","288 usable litres","220 liters","248 usable liters","246 usable litres","288 usable litres","459 usable liters","459 usable liters"]
["Cooling system ","30 litres","25 liters","26.8 liters","28 litres","30 litres","57 liters","57 liters"]
["Engine oil ","15 litres","14.5 liters","13 liters","15 litres","15 litres","26 liters","26 liters"]
["Hydraulic oil ","Tank: 110 litres, total system: 200 litres","Tank: 131 liters, total system: 176 liters","Tank: 91 liters, total system: 148 liters","Tank: 91 litres, total system: 180 litres","Tank: 91 litres, total system: 180 litres","Tank: 134 litres, total system: 250 liters","Tank: 134 litres, total system: 250 liters"]
["Transmission oil ","34 litres","21 liters","27 liters","34 litres","34 litres","45 liters","45 liters"]
["CAB AND CONTROLS"]
["Protection against falling objects (FOPS) ","ISO EN3449","-","ISO EN3449","ISO EN3449","ISO EN3449","ISO EN3449","ISO EN3449"]
["Protection against roll over (ROPS)  ","ISO EN13510","-","ISO EN13510","ISO EN13510","ISO EN13510","ISO EN13510","ISO EN13510"]
["Air flow ","-","-","8.5 m³ / min spread through 17 air vents","-","-","-","-"]
["NOISE AND VIBRATION"]
["Interior noise ","72 LpA as per ISO6595/6396/3744","93 dB(A) ad per ISO 6396","71 dB(A) as per ISO 6595/6396/3744","72 LpA as per ISO6395/6396/3744","72 LpA as per ISO6395/6396/3744","Lpa = 79 dB (A) in compliance with standard ISO 6396:2008","Lpa = 79 dB (A) in compliance with standard ISO 6396:2008"]
["Exterior noise ","71 dB(A) at 15 meters as per SAE J88 SEP80 \n103 LwA according to ISO6395/6396/3744","107 dB(A) ad per ISO 6396","72 dB(A) at 15 meters as per SAE J88 SEP80 \n103 dB (A) according to ISO 6595/6396/3744","71 dB(A) at 15 meters as per SAE J88 SEP80 \n103 LwA according to ISO6395/6396/3744","71 dB(A) at 15 meters as per SAE J88 SEP80 \n103 LwA according to ISO6395/6396/3744","Lwa = 108 dB (A) according to  European Directive 2000/14/EC","Lwa = 108 dB (A) according to  European Directive 2000/14/EC"]
["Vibrations ","air-cushioned seat MSG 95A/732 average 1.4m/s² as per ISO/TR 25398:2006","-","Operator ‘s seat meets the criteria of ISO 7096:2000. The vibrations transmitted do not exceed 0.5 m/s²","air-cushioned seat MSG 95A/732 average 1.4m/s² as per ISO/TR 25398:2006","air-cushioned seat MSG 95A/732 average 1.4m/s² as per ISO/TR 25398:2006","air-cushioned seat MSG 95A/732","air-cushioned seat MSG 95A/732"]
["ELECTRICAL SYSTEM"]
["Batteries ","24V. Batteries 2 x 12V.","24V. Batteries 2 x 12V","24V. Batteries 2 x 12V","24V. Batteries 2 x 12V.","24V. Batteries 2 x 12V.","24V Batteries 2 x 12V","24V Batteries 2 x 12V"]
["Alternator ","65A","70 A","65 A","65A","65A","65A","65A"]